{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sayfa1"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sayfa1","index":0,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[[1,0,1,2],[11,0,11,2]]}
["ANKASTRE KİRİŞ MAKSİMUM SEHİM HESABI "]
["GİRDİ"]
["İsmi","Değeri","Birimi"]
["Kuvvet (F)",100,"N"]
["Uzunluk (l)",4.5,"m"]
["Kesit Genişliği (b)",50,"mm"]
["Kesit Yüksekliği (h)",120,"mm"]
["Malzeme","St",null,null,null,null,"Maksimum Sehim"]
["Elastisite Modülü E",{"$f":"VLOOKUP(B8,A17:B21,2)","v":207},"GPa"]
["Kesit Atalet Momenti",{"$f":"+B6*B7^3/12","v":7200000},"mm4"]
[]
["ÇIKTI"]
["Maksimum Sehim (dmax)",{"$f":"+B4*B5^3/B9/B10/3*1000000","v":2.0380434782608692},"mm",null,"Kesit"]
[null,null,null,null,null,null,null,null,null,"Kesit Atalet Momenti"]
[]
["Malzeme","Elastisite Modülü","Birim"]
["Aluminyum (6061-T6)",71,"GPa"]
["Br",103,"GPa"]
["Cu",119,"GPa"]
["N",210,"GPa"]
["St",207,"GPa"]