{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":3,"images":5,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":20,"n_cols":12,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[null,"Bir Diod için Akım-Voltaj İlişkisi"]
[]
[null,"I","V"]
[null,"(mA)","(Volt)",null,null,null,"A"]
[null,null,null,null,null,{"$f":"LOGEST((B6:B18),(C6:C18))","v":2231745536.2335424},4.5437116281178736E-6]
[null,1E-3,0.23,{"$f":"+LN(B6)","v":-6.9077552789821368},null,"b"]
[null,5.0000000000000001E-3,0.34,{"$f":"+LN(B7)","v":-5.2983173665480363},null,{"$f":"+LN(F5)","v":21.526049867902351}]
[null,0.01,0.38,-4.6051701859880909]
[null,0.02,0.4,-3.912023005428146]
[null,0.05,0.42,-2.9957322735539909]
[null,0.1,0.45,-2.3025850929940455]
[null,0.2,0.5,-1.6094379124341003]
[null,0.5,0.54,-0.69314718055994529]
[null,1,0.56999999999999995,0]
[null,2,0.62,0.69314718055994529]
[null,5,0.64,1.6094379124341003]
[null,10,0.67,2.3025850929940459]
[null,14,0.69,2.6390573296152584,null,null,null,null,null,null,"ln(I)=21.28V-12.1211"]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+EXP(-12.30177)","v":4.5436950012588077E-6}]